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  TEL/WhatsApp: +86 17622605414
Mail: admin@transformercoilwindingmachine.com
    Web:www.transformercoilwindingmachine.com

NAME:ADSKX22-2 Ceiling fan winding machine  
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Specifications：
	Spindle number
	2

	Wire size range
	0.1-1.2mm

	Loop diameter
	200mm

	The max wire spacing
	9.99mm

	Winder width
	100mm

	Max speed
	2200 RPM

	Spindle motor
	Three Phase motor+AC Driver

	Winder motor
	Stepping motor

	Input power
	220V  50HZ/60HZ

	Machine size
	720×950×1300mm

	Package size
	860×1400×1320mm

	Net weight
	180kg

	Gross weight
	220kg


Features:

This Ceiling fan winding machine design of 32 bit controller chip, It’ll be faster and higher reliability.

In Chinese and English display,easy to operation,winding data retention after power failure, not to discarded products。

All the parts for this machine are imported prats,such as:Japan Bearing (NSK、NTN),Japan BANDO belt ，U.S.A GATES belt ，Taiwan Ball screw (TBI)，Taiwan AC Drive and so on.
Fan Winding Machine use two spindle synchronous design, selection of high-power phase motor, making a thick wire around the low-speed torque when larger and more stable. Coupled with high-power stepper motor ,when it rotates will get higher accuracy, so that customers to feel save time,save worker,high production.

Stator Winding Machine suitable for all kinds of  motor stator winding, a variety of ceiling fan stator, pole number stator, locomotives generators.

Advantages：

Ceiling fan winding machine design of 32 bit controller chip, It’ll be faster and higher reliability.

In Chinese and English display,easy to operation,winding data retention after power failure, not to discarded products。

All the parts for this machine are imported prats,such as:Japan Bearing (NSK、NTN),Japan BANDO belt ，U.S.A  GATES belt ，Taiwan Ball screw (TBI)，Taiwan AC Drive and so on.

Warranty period 1 year

The technicians are experienced

APPLICATION:

The ADSKX22-2 Ceiling Fan Winding Machine is mainly used as ideal equipment for the outer winding of stator coils, including ceiling fan stators, water pump stators, and magneto stators—specializing in meeting the winding needs of ceiling fan stators while also adapting to other similar stator components.

In the winding process, the ADSKX22-2 Ceiling Fan Winding Machine can automatically complete core actions such as winding, arranging, turning, advancing, and retreating; it also supports the whole arrangement of windings with large wire diameters, effectively solving the challenge of uniform arrangement for thick wires in stator winding.

Equipped with microcomputer CNC control, this machine enables easy data setting (e.g., winding turns, arrangement density) for quick adaptation to different ceiling fan stator specifications. Its performance is stable and reliable during long-term operation, and it can save 7-15% of enameled wire by optimizing winding paths—reducing material waste while ensuring the quality of ceiling fan stator windings.
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PRACTICAL APPLICATION :

Training for Customers to Operate ADSKX22-2 Ceiling Fan Winding Machine

1.All service engineers with 10 years of experience have received special technical training, including specialized expertise in the ADSKX22-2 Ceiling Fan Winding Machine, enabling them to effectively handle various breakdown issues specific to this ceiling fan stator winding equipment, such as stator alignment errors, wire tension fluctuations, or CNC program malfunctions.

2.We guide users to accurately operate and maintain the ADSKX22-2 Ceiling Fan Winding Machine—with focused attention to its microcomputer control panel operations, stator clamping adjustments, wire arrangement parameter settings, and routine maintenance of key components like winding spindles and wire guides—while providing free consultation about the production process technology related to electronic ceiling fan winding, including optimal winding sequences for different ceiling fan stator models.

3.To ensure the ADSKX22-2 Ceiling Fan Winding Machine operates normally, we conduct dedicated training on its CNC programming, automatic winding function activation, troubleshooting of common issues, and preventive maintenance protocols through English manuals, model-specific instructional videos, and real-time online guidance—all tailored to the unique features of this specialized ceiling fan winding equipment.
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PACKAGING:

Packaging Material: Carton/Wooden case with foam inside.
1.General package(Paper carton or plastic bag): For small euipped parts for  Ceiling fan winding machine       

, Package it with form and pack paper to guarantee unbroken during the transport.
2.Wooden case package: For larger scale  Ceiling fan winding machine ,we have special skilled carpenter, who would make the proper wooden case with exact thickness,density,length. The up arrow ↑marked on the  outer wooden case. Buffer material would be put in the wooden case to prevent crack and shock.
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FACTORY:

We, KIOXIA LIGHT RING EQUIPMENT GROUP CO.,LTD., have been experts in winding machine lines for 28 years, with our specialized product range including advanced equipment like the ADSKX22-2 Ceiling Fan Winding Machine—a precision-engineered system designed for efficient ceiling fan stator winding, embodying our technical expertise in specialized winding solutions for electrical components.

Our KIOXIA LIGHT RING brand holds authoritative certifications and recognitions, including ISO9001:2015, CE approvals, multiple machine patents (encompassing key innovations in models like the ADSKX22-2 Ceiling Fan Winding Machine), and the official designation of "high-tech enterprise" by the government. These credentials fully validate the reliability, performance, and technical excellence of our entire product range, reinforcing our commitment to delivering advanced winding solutions for diverse applications, including specialized ceiling fan production needs.
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KIOXIA LIGHT RING EQUIPMENT GROUP CO.,LTD.
Add: Building G, No.209 Zhonghuan East Road, Free Trade Zone (Airport Economic Zone), Tianjin

